8 cylinders firing orders:  In-line engines & 90 deg V
90 degree banked V8 engines can also be adjusted using the TDC method. A very convenient way to do 8 cylinders without constantly turning the engine over 8 times to do all the tappets if your using the overlap method and much less labour intensive than the ICEO method that so many seem to love. I have listed 7 firing orders that I am aware off, if you have another one let me know & I will add it to the list below.

Firing order  1-3-7-2-6-5-4-8
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set Ex
	Set Ex
	Set In
	Set In
	on overlap
	Set Ex
	Set In

	TDC compression #6
	on overlap
	Set In
	Set In
	Set Ex
	Set Ex
	Set In & Ex
	Set In
	Set Ex


Firing order 1-8-4-3-6-5-7-2
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set In
	Set Ex
	Set Ex
	Set In
	on overlap
	Set In
	Set Ex

	TDC compression #6
	on overlap
	Set Ex
	Set In
	Set In
	Set Ex
	Set In & Ex
	Set Ex
	Set In


Firing order 1-8-7-3-6-5-4-2  The 4/7 swap for the Chev
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set In
	Set Ex
	Set In
	Set In
	on overlap
	Set Ex
	Set Ex

	TDC compression #6
	on overlap
	Set Ex
	Set In
	Set Ex
	Set Ex
	Set In & Ex
	Set In
	Set In


Firing order 1-2-7-8-4-5-6-3
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set Ex
	Set In
	on overlap
	Set In
	Set In
	Set Ex
	Set Ex

	TDC compression #4
	on overlap
	Set In
	Set Ex
	Set In & Ex
	Set Ex
	Set Ex
	Set In
	Set In


Firing order 1-5-4-2-6-3-7-8
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set Ex
	Set In
	Set Ex
	Set Ex
	on overlap
	Set In
	Set In

	TDC compression #6
	on overlap
	Set In
	Set Ex
	Set In
	Set In
	Set In & Ex
	Set Ex
	Set Ex


Firing order 1-5-4-8-6-3-7-2
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set In
	Set In
	Set Ex
	Set Ex
	on overlap
	Set In
	Set Ex

	TDC compression #6
	on overlap
	Set Ex
	Set Ex
	Set In
	Set In
	Set In & Ex
	Set Ex
	Set In


Firing order 1-8-7-2-6-5-4-3
	8 cyl Engine
	No.1
	No.2
	No.3
	No.4
	No.5
	No.6
	No.7
	No.8

	TDC compression #1
	Set In & Ex
	Set Ex
	Set In
	Set In
	Set In
	on overlap
	Set Ex
	Set Ex

	TDC compression #6
	on overlap
	Set In
	Set Ex
	Set Ex
	Set Ex
	Set In & Ex
	Set In
	Set In


 
